AnalyzeSuspend v4.5
helmuth-N24-25BU 4.10.0-rc6+ mem January 31 2017, 07:21:26 PM

Total Suspend Time: 944 ms | Total Resume Time: 888 ms

Kernel Suspend: 944.164 ms | Firmware Suspend: 0.000 ms | Firmware Resume: 1.273 ms | Kernel Resume: 886.649 ms

00:07 {system}
00:04 {i8042 aux}
00:01 {rtc_cmos}
00:00 {system}
input20 {input}
host1 {scsi}
host0 {scsi}
phy0-led {leds}
snd-soc-dummy {snd-soc-dummy}
i8042 {i8042}
usb4 {usb}
PNP0C14:00 {platform}
input4::scrolllock {leds}
PNP0C0C:00 {button}
microcode {platform}
intel_backlight {backlight}
input4::numlock {leds}
0000:00:02.0 {i915}
LNXTHERM:00 {thermal}
0000:03:00.1 {r8169}
0000:03:00.0 {rtsx_pci}
usb2 {usb}
usb3 {usb}
usb1 {usb}
0000:00:1c.2 {pcieport}
0000:00:1c.0 {pcieport}
0000:00:1c.5 {pcieport}
0000:01:00.0 {xhci_hcd}
serial8250 {serial8250}
PNP0C09:00 {ec}
reg-dummy {reg-dummy}
alarmtimer {alarmtimer}
input4::capslock {leds}
0000:04:00.0 {nvme}
0000:02:00.0 {iwlwifi}
0000:00:17.0 {ahci}
tuxedo_wmi {tuxedo_wmi}
rtsx_pci_ms.0 {rtsx_pci_ms}
coretemp.0 {coretemp}
rtsx_pci_sdmmc.0 {rtsx_pci_sdmmc}
hdaudioC0D0 {snd_hda_codec_realtek}
hdaudioC0D2 {snd_hda_codec_hdmi}
rtc0 {rtc}
input2 {input}
input3 {input}
input4 {input}
phy0 {ieee80211}
ata1
ata2
input19 {input}
serio4 {serio}
0000:00:1f.2 {intel_pmc_core}
0000:00:1f.0 {pci}
serio0 {atkbd}
serio1 {serio}
serio2 {psmouse}
0000:00:14.0 {xhci_hcd}
0000:00:1d.0 {pcieport}
0000:00:16.0 {mei_me}
tuxedo::airplane {leds}
1-5 {usb}
1-6 {usb}
input18 {input}
0000:00:1f.3 {snd_hda_intel}
rfkill1 {rfkill}
rfkill0 {rfkill}
input10 {input}
input11 {input}
input14 {input}
input15 {input}
input16 {input}
0000:00:02.0 {i915}
syscore_suspend
acpi_pm_prepare
CPU_OFF[1]
CPU_OFF[2]
CPU_OFF[3]
0000:03:00.1 {r8169}
0000:03:00.0 {rtsx_pci}
0000:00:1d.0 {pcieport}
0000:04:00.0 {nvme}
PNP0C09:00 {ec}
0000:00:1f.2 {intel_pmc_core}
0000:00:1c.0 {pcieport}
0000:00:1f.0 {pci}
0000:00:1c.2 {pcieport}
0000:00:08.0 {pci}
0000:00:1f.4 {pci}
0000:00:1f.3 {snd_hda_intel}
0000:02:00.0 {iwlwifi}
0000:00:17.0 {ahci}
0000:00:14.0 {xhci_hcd}
0000:01:00.0 {xhci_hcd}
0000:00:14.2 {intel_pch_thermal}
0000:00:16.0 {mei_me}
0000:00:02.0 {i915}
0000:00:00.0 {pci}
0000:00:1c.5 {pcieport}
ttyS5 {tty}
00:07 {system}
00:05 {system}
00:04 {i8042 aux}
00:03 {i8042 kbd}
00:01 {rtc_cmos}
00:00 {system}
device:2f {acpi}
device:2e {acpi}
device:2d {acpi}
device:2c {acpi}
device:2a {acpi}
ttyS0 {tty}
ttyS3 {tty}
usb4-port2 {usb}
input17 {input}
ttyS2 {tty}
PNP0A08:00 {acpi}
usb1-port1 {usb}
INT344A:00 {acpi}
pcmC0D7p {sound}
device:29 {acpi}
device:28 {acpi}
device:27 {acpi}
device:26 {acpi}
device:25 {acpi}
device:23 {acpi}
device:22 {acpi}
device:21 {acpi}
tty15 {tty}
ep_83
drm_dp_aux0 {drm_dp_aux_dev}
memory58 {memory}
hpet {misc}
drm_dp_aux1 {drm_dp_aux_dev}
1-6:1.1 {uvcvideo}
pnp0
PNP0C0E:00 {platform}
tty6 {tty}
tty4 {tty}
tty2 {tty}
tty1 {tty}
tty0 {tty}
thermal_zone3 {thermal}
node0 {node}
INT3448:00 {acpi}
thermal_zone0 {thermal}
tty8 {tty}
LNXVIDEO:00 {video}
7:5 {bdi}
zero {mem}
ep_81
7:0 {bdi}
PNP0C0C:00 {platform}
0000:00:00.0 {pci}
7:1 {bdi}
port {mem}
mei::f908627d-13bf-4a04-b91f-a64e9245323d:01 {mei}
mei::8e6a6715-9abc-4043-88ef-9e39c6f63e0f:01 {mei}
tty62 {tty}
tty60 {tty}
input4::numlock {leds}
ttyS20 {tty}
ttyS22 {tty}
ttyS23 {tty}
ttyS25 {tty}
ttyS26 {tty}
ttyS27 {tty}
ttyS29 {tty}
LNXTHERM:00 {thermal}
writeback {workqueue}
memory152 {memory}
memory153 {memory}
memory155 {memory}
memory156 {memory}
memory158 {memory}
vcs6 {vc}
memory67 {memory}
PNP0100:00 {acpi}
memory65 {memory}
memory64 {memory}
memory63 {memory}
memory62 {memory}
memory60 {memory}
cpu_dma_latency {misc}
memory69 {memory}
vcs2 {vc}
tty55 {tty}
tuxedo_wmi {tuxedo_wmi}
tty54 {tty}
7:4 {bdi}
tty52 {tty}
tty51 {tty}
PNP0C09:00 {platform}
sys_sync
loop0 {block}
tty19 {tty}
memory259 {memory}
0000:02:00.0 {iwlwifi}
memory
memory253 {memory}
memory251 {memory}
memory250 {memory}
memory257 {memory}
memory256 {memory}
memory254 {memory}
fb0 {graphics}
vcs7 {vc}
rfkill {misc}
PNP0C04:00 {acpi}
0000:00:14.0 {xhci_hcd}
0000:00:14.2 {intel_pch_thermal}
rtsx_pci_ms.0 {rtsx_pci_ms}
ep_82
workqueue
INT3470:00 {acpi}
bus.0 {platform Fixed MDIO}
1:12 {bdi}
1:13 {bdi}
device:73 {acpi}
1:11 {bdi}
7:2 {bdi}
7:3 {bdi}
1:14 {bdi}
1:15 {bdi}
card0-eDP-1 {drm}
rtsx_pci_sdmmc.0 {rtsx_pci_sdmmc}
hdaudioC0D0 {snd_hda_codec_realtek}
hdaudioC0D2 {snd_hda_codec_hdmi}
INT344B:00 {acpi}
input2 {input}
input0 {input}
input4 {input}
intel_bts {event_source}
INT343D:00 {acpi}
usb3-port1 {usb}
ACPI0003:00 {platform}
ata1 {ata_port}
ata2 {ata_port}
loop5 {block}
ABBC0F6D-8EA1-11D1-00A0-C90629100000 {wmi}
serio4 {serio}
serio0 {atkbd}
serio1 {serio}
serio2 {psmouse}
id {dmi}
hwC0D0 {sound}
device:69 {acpi}
snd-soc-dummy {snd-soc-dummy}
device:63 {acpi}
device:62 {acpi}
device:60 {acpi}
device:67 {acpi}
device:66 {acpi}
device:65 {acpi}
link2 {ata_link}
mei::42b3ce2f-bd9f-485a-96ae-26406230b1ff:01 {mei}
memory208 {memory}
suspend_console
memory6 {memory}
memory4 {memory}
memory181 {memory}
memory186 {memory}
memory184 {memory}
device:6b {acpi}
memory188 {memory}
memory9 {memory}
device:6d {acpi}
PNP0C0F:05 {acpi}
memory_bandwidth {misc}
serial8250 {serial8250}
ram12 {block}
memory200 {memory}
memory202 {memory}
memory204 {memory}
memory206 {memory}
memory160 {memory}
memory163 {memory}
memory165 {memory}
memory167 {memory}
memory59 {memory}
IMPJ0003:00 {acpi}
intel-rapl {powercap}
memory14 {memory}
memory15 {memory}
memory13 {memory}
memory10 {memory}
memory11 {memory}
input20 {input}
lo {net}
INT3445:00 {acpi}
platform
memory118 {memory}
memory114 {memory}
memory116 {memory}
memory110 {memory}
memory112 {memory}
memory56 {memory}
memory57 {memory}
cooling_device4 {thermal}
ttyS7 {tty}
0000:00:16.0 {mei_me}
usb2-port2 {usb}
usb2-port6 {usb}
usb2-port4 {usb}
pcspkr {platform}
mcelog {misc}
mem {mem}
device:31 {acpi}
device:33 {acpi}
device:35 {acpi}
device:37 {acpi}
device:38 {acpi}
device:39 {acpi}
vga_arbiter {misc}
PNP0C14:00 {platform}
mei::8c2f4425-77d6-4755-aca3-891fdbc66a58:01 {mei}
input4::scrolllock {leds}
msr {event_source}
memory169 {memory}
memstick0 {memstick_host}
ttyS1 {tty}
ACPI000C:00 {platform}
container
0000:04 {pci_bus}
pcmC0D8p {sound}
0000:01 {pci_bus}
0000:00 {pci_bus}
0000:03 {pci_bus}
0000:02 {pci_bus}
clocksource0 {clocksource}
i2c-2 {i2c-dev}
i2c-0 {i2c-dev}
i2c-1 {i2c-dev}
0000:03:00.1 {r8169}
0000:03:00.0 {rtsx_pci}
tty57 {tty}
device:3a {acpi}
device:3b {acpi}
device:3c {acpi}
device:3d {acpi}
device:3f {acpi}
tty50 {tty}
index2
index3
loop7 {block}
loop6 {block}
INT343E:00 {acpi}
LNXCPU:07 {acpi}
memory234 {memory}
253:0 {bdi}
PNP0000:00 {acpi}
PNP0C02:02 {acpi}
regulator.0 {regulator}
event10 {input}
nvme0n1 {block}
mei::01e88543-8050-4380-9d6f-4f9cec704917:01 {mei}
PNP0C02:05 {acpi}
isa
ttyS31 {tty}
PNP0C02:04 {acpi}
memory124 {memory}
memory126 {memory}
memory120 {memory}
memory122 {memory}
memory53 {memory}
memory51 {memory}
memory128 {memory}
memory54 {memory}
memory55 {memory}
reg-dummy {reg-dummy}
mei::5565a099-7fe2-45c1-a22b-d7e9dfea9a2e:01 {mei}
freeze_kernel_threads
i8042 {i8042}
input4::capslock {leds}
INT3440:00 {acpi}
0000:04:00.0 {nvme}
1-0:1.0 {hub}
card0 {sound}
event11 {input}
memory239 {memory}
memory238 {memory}
usb1-port9 {usb}
usb1-port8 {usb}
memory5 {memory}
memory231 {memory}
memory233 {memory}
memory232 {memory}
cpu2 {processor}
cpu3 {processor}
memory237 {memory}
broadcast {clockevents}
memory7 {memory}
ep_03
memory0 {memory}
memory1 {memory}
memory3 {memory}
network_latency {misc}
pcmC0D0p {sound}
memory248 {memory}
memory244 {memory}
memory245 {memory}
memory246 {memory}
memory240 {memory}
memory241 {memory}
memory243 {memory}
mei::dba4d603-d7ed-4931-8823-17ad585705d5:01 {mei}
card0-DP-1 {drm}
ttyS9 {tty}
pci0000:00
device:0a {acpi}
device:0c {acpi}
device:0b {acpi}
device:0e {acpi}
device:0f {acpi}
vcsa7 {vc}
vcsa4 {vc}
vcsa2 {vc}
dev2.0 {ata_device}
vcsa1 {vc}
0000:00:1f.3 {snd_hda_intel}
0000:00:1f.2 {intel_pmc_core}
0000:00:1f.0 {pci}
0000:00:1f.4 {pci}
usb1-port5 {usb}
ecryptfs-1 {bdi}
usb1-port4 {usb}
0000:00:1d.0 {pcieport}
device:09 {acpi}
device:08 {acpi}
usb1-port6 {usb}
vcs5 {vc}
device:01 {acpi}
device:00 {acpi}
device:03 {acpi}
device:02 {acpi}
device:05 {acpi}
device:07 {acpi}
enp3s0f1 {net}
cpu0 {processor}
breakpoint {event_source}
memory236 {memory}
controlC0 {sound}
INT33A2:00 {acpi}
event3 {input}
snapshot {misc}
event0 {input}
rfkill0 {rfkill}
device:74 {acpi}
device:70 {acpi}
device:71 {acpi}
device:72 {acpi}
device:5c {acpi}
memory96 {memory}
memory94 {memory}
memory95 {memory}
memory92 {memory}
memory93 {memory}
INT0000:00 {acpi}
random {mem}
memory98 {memory}
mei0 {mei}
hwmon2 {hwmon}
hwmon1 {hwmon}
hwmon0 {hwmon}
memory195 {memory}
memory196 {memory}
memory197 {memory}
memory190 {memory}
memory192 {memory}
memory193 {memory}
cache
memory198 {memory}
MSFT0001:00 {acpi}
media0 {media}
memory209 {memory}
regulatory.0 {platform}
memory178 {memory}
memory179 {memory}
memory270 {memory}
memory172 {memory}
memory171 {memory}
memory177 {memory}
memory174 {memory}
memory175 {memory}
input19 {input}
ram10 {block}
INT3449:00 {acpi}
INT3447:00 {acpi}
vcsa {vc}
pcmC0D0c {sound}
machinecheck
memory183 {memory}
memory151 {memory}
device:4e {acpi}
device:4d {acpi}
device:4f {acpi}
device:4a {acpi}
0:44 {bdi}
device:4c {acpi}
device:4b {acpi}
usb2 {usb}
microcode {misc}
usb3 {usb}
ram8 {block}
ram9 {block}
ram5 {block}
ram6 {block}
ram0 {block}
ram1 {block}
ram2 {block}
ram3 {block}
0000:00:02.0 {i915}
event12 {input}
thermal_zone2 {thermal}
event13 {input}
device:44 {acpi}
device:46 {acpi}
device:41 {acpi}
device:40 {acpi}
device:43 {acpi}
device:42 {acpi}
device:48 {acpi}
nvme0n1p3 {block}
thermal_zone1 {thermal}
tun {misc}
0000:01:00.0 {xhci_hcd}
2-0:1.0 {hub}
fbcon {graphics}
tty40 {tty}
tty41 {tty}
tty42 {tty}
tty44 {tty}
tty46 {tty}
tty47 {tty}
tty49 {tty}
usb4-port1 {usb}
dev1.0 {ata_device}
0000:00:17.0 {ahci}
dm-0 {block}
memory136 {memory}
memory137 {memory}
memory135 {memory}
memory49 {memory}
memory133 {memory}
memory130 {memory}
memory45 {memory}
memory44 {memory}
memory47 {memory}
memory41 {memory}
memory40 {memory}
memory43 {memory}
memory42 {memory}
tty13 {tty}
tty35 {tty}
tty37 {tty}
tty30 {tty}
tty33 {tty}
tty32 {tty}
tty39 {tty}
tty12 {tty}
ptmx {tty}
1:8 {bdi}
memory228 {memory}
memory229 {memory}
usb1-port3 {usb}
memory222 {memory}
memory220 {memory}
memory221 {memory}
memory226 {memory}
memory224 {memory}
memory38 {memory}
memory39 {memory}
card0-HDMI-A-2 {drm}
card0-HDMI-A-1 {drm}
memory32 {memory}
memory34 {memory}
memory36 {memory}
INT3446:00 {acpi}
usb1-port2 {usb}
null {mem}
vtcon0 {vtconsole}
PNP0C0F:04 {acpi}
PNP0C0F:07 {acpi}
PNP0C0F:06 {acpi}
PNP0C0F:01 {acpi}
PNP0C0F:00 {acpi}
PNP0C0F:02 {acpi}
mei::309dcde8-ccb1-4062-8f78-600115a34327:01 {mei}
freeze_processes
XXXX0000:01 {acpi}
XXXX0000:00 {acpi}
1-5 {usb}
tty17 {tty}
INT33E1:00 {acpi}
PNP0C02:01 {acpi}
PNP0C02:00 {acpi}
LNXCPU:05 {acpi}
LNXCPU:04 {acpi}
LNXCPU:03 {acpi}
LNXCPU:02 {acpi}
LNXCPU:01 {acpi}
LNXCPU:00 {acpi}
ram14 {block}
vcsa3 {vc}
tty16 {tty}
mmc0 {mmc_host}
ecryptfs {misc}
event8 {input}
event9 {input}
event4 {input}
event5 {input}
event1 {input}
device:18 {acpi}
device:12 {acpi}
device:13 {acpi}
device:10 {acpi}
device:11 {acpi}
device:16 {acpi}
device:17 {acpi}
device:15 {acpi}
serio3 {serio}
clocksource
hci0 {bluetooth}
intel_pt {event_source}
console {tty}
PNP0C0D:00 {platform}
network_throughput {misc}
SYN1217:00 {acpi}
host1 {scsi_host}
host0 {scsi_host}
machinecheck3 {machinecheck}
machinecheck0 {machinecheck}
machinecheck1 {machinecheck}
LNXSYBUS:00 {acpi}
phy0-led {leds}
INT0E0C:00 {platform}
1:0 {bdi}
1:3 {bdi}
1:4 {bdi}
1:5 {bdi}
1:7 {bdi}
ABBC0F6C-8EA1-11D1-00A0-C90629100000 {wmi}
device:1c {acpi}
loop-control {misc}
device:1a {acpi}
device:1f {acpi}
device:1d {acpi}
device:1e {acpi}
acpi_suspend_begin
INT33A1:00 {acpi}
ttyS15 {tty}
ttyS16 {tty}
ttyS11 {tty}
ttyS10 {tty}
ttyS13 {tty}
ttyS18 {tty}
memory267 {memory}
memory265 {memory}
memory263 {memory}
memory149 {memory}
memory147 {memory}
memory146 {memory}
memory144 {memory}
memory142 {memory}
memory141 {memory}
memory140 {memory}
memory75 {memory}
memory77 {memory}
memory70 {memory}
memory72 {memory}
memory73 {memory}
intel-rapl:0 {powercap}
memory79 {memory}
1-5:1.0 {btusb}
cooling_device1 {thermal}
cooling_device0 {thermal}
cooling_device3 {thermal}
cooling_device2 {thermal}
clockevent0 {clockevents}
clockevent2 {clockevents}
fixed-0 {mdio_bus}
memory89 {memory}
memory88 {memory}
vtcon1 {vtconsole}
memory81 {memory}
memory80 {memory}
memory82 {memory}
memory84 {memory}
memory87 {memory}
memory86 {memory}
ttyprintk {tty}
kvm {misc}
0000:00:1c.2 {pcieport}
0000:00:1c.0 {pcieport}
hw_random {misc}
INT0800:00 {platform}
tty10 {tty}
BAT0 {power_supply}
software {event_source}
device:57 {acpi}
device:54 {acpi}
device:55 {acpi}
device:52 {acpi}
device:53 {acpi}
device:51 {acpi}
device:59 {acpi}
alarmtimer {alarmtimer}
4-0:1.0 {hub}
INT33D0:00 {acpi}
coretemp.0 {coretemp}
memory260 {memory}
memory261 {memory}
intel-rapl:0:0 {powercap}
intel-rapl:0:2 {powercap}
platform-framebuffer.0 {platform}
PNPC000:00 {acpi}
INT3420:00 {acpi}
mei::55213584-9a29-4916-badf-0fb7ed682aeb:01 {mei}
LNXPWRBN:00 {button}
device:5e {acpi}
device:5b {acpi}
memory268 {memory}
pcmC0D3p {sound}
device:5a {acpi}
PNP0B00:00 {acpi}
mice {input}
memory269 {memory}
FPNT_DIS:00 {acpi}
usb1 {usb}
full {mem}
usb1-port10 {usb}
usb1-port12 {usb}
LNXSYSTM:00 {acpi}
mouse0 {input}
device-mapper {misc}
hwC0D2 {sound}
autofs {misc}
rtc0 {rtc}
PNP0C0A:00 {platform}
ram15 {block}
kmsg {mem}
phy0 {ieee80211}
INT340E:00 {acpi}
mei::3c4852d6-d47b-4f46-b05e-b5edc1aa440e:01 {mei}
mei::082ee5a7-7c25-470a-9643-0c06f0466ea1:00 {mei}
memory132 {memory}
tty26 {tty}
tty27 {tty}
tty25 {tty}
tty22 {tty}
tty23 {tty}
tty20 {tty}
tty28 {tty}
wlp2s0 {net}
INT3443:00 {acpi}
ABBC0F6B-8EA1-11D1-00A0-C90629100000 {wmi}
tuxedo::airplane {leds}
STU0604:00 {acpi}
cooling_device5 {thermal}
AC {power_supply}
video0 {video4linux}
memory219 {memory}
memory217 {memory}
memory215 {memory}
memory213 {memory}
memory212 {memory}
memory211 {memory}
input10 {input}
rfkill1 {rfkill}
memory138 {memory}
input11 {input}
intel_backlight {backlight}
input14 {input}
input18 {input}
nvme0 {nvme}
memory109 {memory}
input16 {input}
memory103 {memory}
memory102 {memory}
memory101 {memory}
memory100 {memory}
memory107 {memory}
memory105 {memory}
memory104 {memory}
-900ms
-800ms
-700ms
-600ms
-500ms
-400ms
-300ms
-200ms
-100ms
Suspend
00:08 {system}
00:07 {system}
00:04 {i8042 aux}
00:03 {i8042 kbd}
00:01 {rtc_cmos}
00:00 {system}
0000:00:1f.4 {pci}
input20 {input}
host1 {scsi}
host0 {scsi}
snd-soc-dummy {snd-soc-dummy}
0000:00:08.0 {pci}
i8042 {i8042}
PNP0C0E:00 {platform}
0000:03:00.1 {r8169}
input4::scrolllock {leds}
microcode {platform}
intel_backlight {backlight}
0000:00:02.0 {i915}
regulatory.0 {platform}
LNXTHERM:00 {thermal}
usb4 {usb}
0000:03:00.0 {rtsx_pci}
usb2 {usb}
usb3 {usb}
usb1 {usb}
0000:00:1c.2 {pcieport}
0000:00:1c.0 {pcieport}
0000:00:1c.5 {pcieport}
0000:01:00.0 {xhci_hcd}
INT0800:00 {platform}
serial8250 {serial8250}
reg-dummy {reg-dummy}
alarmtimer {alarmtimer}
0000:04:00.0 {nvme}
platform-framebuffer.0 {platform}
0000:02:00.0 {iwlwifi}
0000:00:17.0 {ahci}
0000:00:14.0 {xhci_hcd}
rtsx_pci_ms.0 {rtsx_pci_ms}
0000:00:14.2 {intel_pch_thermal}
LNXPWRBN:00 {button}
coretemp.0 {coretemp}
bus.0 {platform Fixed MDIO}
rtsx_pci_sdmmc.0 {rtsx_pci_sdmmc}
hdaudioC0D0 {snd_hda_codec_realtek}
hdaudioC0D2 {snd_hda_codec_hdmi}
rtc0 {rtc}
input2 {input}
input3 {input}
input0 {input}
input1 {input}
input4 {input}
phy0 {ieee80211}
ata1
ata2
0000:00:00.0 {pci}
input19 {input}
0000:00:1f.3 {snd_hda_intel}
0000:00:1f.2 {intel_pmc_core}
0000:00:1f.0 {pci}
serio0 {atkbd}
serio1 {serio}
serio2 {psmouse}
serio3 {serio}
tuxedo_wmi {tuxedo_wmi}
0000:00:1d.0 {pcieport}
0000:00:16.0 {mei_me}
tuxedo::airplane {leds}
1-5 {usb}
1-6 {usb}
serio4 {serio}
rfkill1 {rfkill}
input10 {input}
input11 {input}
input14 {input}
input15 {input}
input17 {input}
hpet {misc}
00:05 {system}
00:03 {i8042 kbd}
urandom {mem}
device:2c {acpi}
memory106 {memory}
intel_bts {event_source}
pcmC0D7p {sound}
device:28 {acpi}
hwC0D0 {sound}
snd-soc-dummy {snd-soc-dummy}
tty30 {tty}
i8042 {i8042}
PNP0C0E:00 {button}
tty7 {tty}
tty2 {tty}
thermal_zone3 {thermal}
thermal_zone2 {thermal}
thermal_zone0 {thermal}
LNXVIDEO:00 {video}
memory164 {memory}
INT3F0D:00 {acpi}
0000:00:00.0 {pci}
port {mem}
tty62 {tty}
tty60 {tty}
ttyS23 {tty}
LNXTHERM:00 {thermal}
full {mem}
usb2 {usb}
usb3 {usb}
memory196 {memory}
memory62 {memory}
device:3d {acpi}
PNP0C09:00 {ec}
index0
0000:02:00.0 {iwlwifi}
memory252 {memory}
FPNT_DIS:00 {acpi}
memory257 {memory}
fb0 {graphics}
bus.0 {platform Fixed MDIO}
rtsx_pci_sdmmc.0 {rtsx_pci_sdmmc}
INT344B:00 {acpi}
input3 {input}
serio2 {psmouse}
device:26 {acpi}
device:61 {acpi}
0000:00:16.0 {mei_me}
device:66 {acpi}
device:64 {acpi}
link2
tty12 {tty}
tty16 {tty}
tty14 {tty}
tty19 {tty}
memory8 {memory}
device:6e {acpi}
ACPI0003:00 {ac}
acpi_pm_end
vtcon0 {vtconsole}
memory_bandwidth {misc}
tty {tty}
memory203 {memory}
INT33A1:00 {acpi}
ram12 {block}
ram10 {block}
event11 {input}
input20 {input}
platform
memory114 {memory}
memory111 {memory}
memory35 {memory}
memory57 {memory}
usb2-port1 {usb}
usb2-port6 {usb}
pcspkr {platform}
lightnvm {misc}
vga_arbiter {misc}
pm_notifier_call_chain
input4::scrolllock {leds}
memory169 {memory}
MSFT0003:00 {acpi}
i2c-4 {i2c}
0000:03:00.1 {r8169}
tty53 {tty}
tty51 {tty}
index3
loop0 {block}
tty58 {tty}
machinecheck
253:0 {bdi}
PNP0C02:02 {acpi}
regulator.0 {regulator}
ETD0403:00 {acpi}
ttyS30 {tty}
memory123 {memory}
memory52 {memory}
LNXCPU:03 {acpi}
memory128 {memory}
memory54 {memory}
input4::capslock {leds}
INT3440:00 {acpi}
0000:04:00.0 {nvme}
usb1-port8 {usb}
tuxedo_wmi {tuxedo_wmi}
usb1-port6 {usb}
cpu3 {processor}
coretemp.0 {coretemp}
ep_02
memory248 {memory}
memory243 {memory}
pci0000:00
resume_console
vcsa6 {vc}
vcsa4 {vc}
vcsa5 {vc}
vcsa2 {vc}
ecryptfs-1 {bdi}
usb1-port4 {usb}
device:03 {acpi}
device:05 {acpi}
device:07 {acpi}
enp3s0f1 {net}
event3 {input}
device:74 {acpi}
ttyS4 {tty}
ttyS7 {tty}
ttyS2 {tty}
memory98 {memory}
hwmon3 {hwmon}
memory208 {memory}
memory178 {memory}
memory179 {memory}
memory152 {memory}
device:4e {acpi}
device:4c {acpi}
microcode {platform}
memory155 {memory}
cpu1 {processor}
ram9 {block}
ram4 {block}
device-mapper {misc}
ram2 {block}
memory10 {memory}
device:45 {acpi}
device:47 {acpi}
device:49 {acpi}
memory241 {memory}
memory189 {memory}
memory60 {memory}
tty42 {tty}
tty44 {tty}
memory68 {memory}
memory13 {memory}
dm-0 {block}
wlp2s0 {net}
memory47 {memory}
memory267 {memory}
drm_dp_aux0 {drm_dp_aux_dev}
tty39 {tty}
ptmx {tty}
memory228 {memory}
LNXSYBUS:00 {acpi}
memory222 {memory}
INT343D:00 {acpi}
memory226 {memory}
card0-HDMI-A-1 {drm}
PNP0C0F:06 {acpi}
PNP0C0F:01 {acpi}
XXXX0000:00 {acpi}
1-5 {usb}
1-6 {usb}
PNP0C02:04 {acpi}
LNXCPU:01 {acpi}
ecryptfs {misc}
event7 {input}
event5 {input}
tracepoint {event_source}
event0 {input}
device:19 {acpi}
device:10 {acpi}
device:17 {acpi}
device:15 {acpi}
clocksource
memory160 {memory}
memory1 {memory}
SYN1217:00 {acpi}
host1 {scsi}
phy0-led {leds}
INT0E0C:00 {acpi}
1:0 {bdi}
1:7 {bdi}
thaw_processes
ABBC0F6C-8EA1-11D1-00A0-C90629100000 {wmi}
ttyS14 {tty}
node
memory142 {memory}
intel-rapl:0 {powercap}
memory94 {memory}
cooling_device1 {thermal}
memory82 {memory}
memory84 {memory}
0000:00:1c.5 {pcieport}
memory236 {memory}
clockevents
device:56 {acpi}
device:50 {acpi}
device:58 {acpi}
memory76 {memory}
INT33D0:00 {acpi}
memory149 {memory}
memory40 {memory}
memory
device:5f {acpi}
mice {input}
memory140 {memory}
memory250 {memory}
usb1-port11 {usb}
tty23 {tty}
pnp0
1-5:1.1 {usb}
kvm {misc}
memory212 {memory}
memory210 {memory}
memory102 {memory}
memory42 {memory}
memory100 {memory}
memory157 {memory}
0000:00:02.0 {i915}
acpi_pm_finish
CPU_ON[1]
CPU_ON[3]
arch_enable_nonboot_cpus_end
CPU_ON[2]
syscore_resume
PNP0C09:00 {ec}
0000:00:00.0 {pci}
0000:04:00.0 {nvme}
0000:00:1f.3 {snd_hda_intel}
0000:00:1f.2 {intel_pmc_core}
0000:00:1f.0 {pci}
0000:00:1f.4 {pci}
0000:00:1c.2 {pcieport}
0000:02:00.0 {iwlwifi}
0000:00:17.0 {ahci}
0000:00:1d.0 {pcieport}
0000:00:16.0 {mei_me}
0000:03:00.1 {r8169}
0000:03:00.0 {rtsx_pci}
0000:00:02.0 {i915}
0000:00:14.0 {xhci_hcd}
0000:00:1c.0 {pcieport}
0000:00:14.2 {intel_pch_thermal}
0000:00:1c.5 {pcieport}
0000:01:00.0 {xhci_hcd}
0000:00:08.0 {pci}
i8042 {i8042}
Resume
100ms
200ms
300ms
400ms
500ms
600ms
700ms
800ms
suspend prepare
suspend
suspend late
suspend noirq
suspend machine
resume machine
resume noirq
resume early
resume
resume complete
Output files: suspend-170131-192126/helmuth-N24-25BU_mem_dmesg.txt suspend-170131-192126/helmuth-N24-25BU_mem_ftrace.txt suspend-170131-192126/helmuth-N24-25BU_mem.html Analyzing the ftrace data... Timeline Details: test start: 3546.667059 kernel suspend start: 3546.667111 suspend_prepare: 3546.667111 - 3546.678509 (917 devices) suspend: 3546.678509 - 3547.472488 (97 devices) suspend_late: 3547.472488 - 3547.491486 (1 devices) suspend_noirq: 3547.491486 - 3547.531428 (21 devices) suspend_machine: 3547.531428 - 3547.611275 (5 devices) resume_machine: 3547.611275 - 3547.670784 (6 devices) resume_noirq: 3547.670784 - 3547.715411 (22 devices) resume_early: 3547.715411 - 3547.726382 (1 devices) resume: 3547.726382 - 3548.484948 (96 devices) resume_complete: 3548.484948 - 3548.497924 (900 devices) kernel resume end: 3548.497924 test end: 3548.497991 Analyzing the dmesg data... Creating Device Timeline...