Hello,

the idea is the same as in HP-UX.
When we are using Linux, it would be good, to get as close to HP-UX as possible.
We're now using LVM in HP-UX to mirror the Volume groupe vg00

/dev/vg00/lvol4     307200   73329  219390   25% /
--- Logical volumes ---
LV Name                     /dev/vg00/lvol4
VG Name                     /dev/vg00
LV Permission               read/write
LV Status                   available/syncd
Mirror copies               1
Consistency Recovery        MWC
Schedule                    parallel
LV Size (Mbytes)            300
Current LE                  75
Allocated PE                150
Stripes                     0
Stripe Size (Kbytes)        0
Bad block                   off
Allocation                  strict/contiguous
IO Timeout (Seconds)        default

We know, that it is possible to implement RAID 1 in other ways, but it's difficult to support.

 -----Original Message-----
From: 	hopper@omnifarious.mn.org [mailto:hopper@omnifarious.mn.org] 
Sent:	Dienstag, 6. Juni 2000 19:34
To:	HOLGER ZECHA /HP-Germany,om17
Cc:	hopper@omnifarious.mn.org; linux-lvm@msede.com
Subject:	Re: [linux-lvm] LVM 0.8 and reiser filesystem

 << File: Re_ [linux-lvm] LVM 0.TXT >>  << File: Re_ [linux-lvm] LVM 0.TXT >>  << File: Untitled1 >>